[Hooke’s Law](http://www.youtube.com/watch?v=OaiynlvxFbk) Name:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Partner(s):\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_    Course:\_\_\_\_\_\_\_\_\_\_\_\_\_\_    Time:\_\_\_\_\_\_\_\_\_\_\_\_

Purpose: To verify Hooke’s law and determine the spring constants of elastic springs.

Apparatus: 3 springs, pendulum clamp, motion sensor, plumb-line, meter stick, tall lab stand, mass set, and mass hanger.

Theory: Think about stretching a spring. The more stretching force you apply, the more stretch you get. Robert Hooke (1635-1703), a British physicist, discovered this empirical relationship between the restoring force (F) and the stretch (x), known as Hooke's law,
F = - kX.

                                                



According to Hooke's law, the magnitude of the stretching force is given by:

 Stretching Force = (Spring constant) X Stretch.

The stretching force is provided by the added mass. You can also plot Stretching Force VERSUS Stretch. Hooke’s law is verified when there is a linear relationship between Stretching Force & Stretch.

The Spring Constant is given by the slope of the Stretching Force versus Stretch graph.

Procedure:

|  |  |  |  |
| --- | --- | --- | --- |
| 1. Attach the mass hanger to the hard spring and hang it from the pendulum clamp.2. Set up the motion sensor about 50-cm below the bottom of the mass hanger, using a plum-line.3. Connect the motion sensor to the interface (yellow-1, black-2), set the beam to narrow.4. Setting up the Interface for data collection: a. Open **PASCO Capstone** software from the desktop.  b. Click **Hardware Setup** under Tools on the left, click on the interface input where the sensor is connected and select **Motion Sensor II**.  Click **Hardware Setup** again to close it.  c. Double-Click **Digits** under Displays on the right, click Select Measurement, and select **Position.**  5. Click **Record** and record the distance to the bottom of mass hanger from the motion sensor. Stop the data collection.6. Add an appropriate mass to make the spring stretch about 2 cm and measure the distance to the bottom of mass hanger, again, and record it.7. Measure the stretches for other added masses and complete the data table.8. Repeat 1-7 for the other two springs.9. Enter the above data in Excel and for each spring; create two more columns for Stretch (m) and Stretching force (N). Calculate these values and make a single XY scatter Plot Stretching force VS. Stretch for all three springs, and find the spring constant for each spring.10. Attach your data table & plot (Excel) and conclusion (Word).  [SAMPLE DATA](file:///C%3A%5CUsers%5Cmahesp%5CDownloads%5CHooke.xlsx) |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |