**Resistivity** [**RESISTANCE**](http://hyperphysics.phy-astr.gsu.edu/hbase/electric/resis.html)                  Name:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Purpose I: To investigate the resistance of metal wires using a [digital multi meter](http://www.youtube.com/watch?v=bF3OyQ3HwfU) (DMM).

Apparatus: DMM, one long metal (nichrome) wire, connector box, micrometer, and meter stick.

Theory: Resistance, R of a metal wire of length *L* and cross-sectional area *A* is given by:

olandr2

The plot of R versus L will yield a slope of *ρ/A.* Knowing A, the resistivity can be determined.

Procedure:

Variation of resistance with length:

1. Set the DMM to measure resistances and connect it to the connector box.
2. Connect one end of the long metal wire to one of the terminals of the connector box.
3. Measure 10 cm length of wire, (do not cut the wire) and connect it to the other terminal so that there is exactly 10 cm of wire between the terminals.
4. Record the resistance value and repeat the above procedure for other lengths: 20, 30, 40, 50, 60, 70, 80, 90, 100 cm.
5. Plot a graph, R versus L, determine its slope, and attach the graph to your report.
6. Measure the diameter of the wire with a micrometer, calculate the cross-sectional area, and calculate the resistivity of the metal.

Variation of resistance with diameter:

1. Fold the wire into half and then again half to make 4 equal pieces.
2. Measure the resistance of one fold, two folds, three folds, and four folds.
3. Tabulate your data, plot an appropriate graph, and see what happens.
4. Add an appropriate trend line, and obtain resistivity from your fit.
5. Attach your graph to the report.

DATA  
  
Variation of resistance with length:

Slope of R versus L, graph:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Diameter of wire = \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_    Cross-Sectional area of wire =\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Experimental resistivity of wire = \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Accepted resistivity of wire = 1.00 x 10-4 ohm.cm. % Error = \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Variation of resistance with diameter:

Coefficient of the fit = \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Length of wire = \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_    Cross-Sectional area (for 1 fold) =\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Experimental resistivity of wire = \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_


Accepted resistivity of wire = 1.00 x 10-4 ohm.cm.

                                    % Error = \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_


Conclusion for Purpose I:

Purpose II: To investigate various combinations of resistors.

Apparatus: Two resistors, DMM (digital multimeter), and 5-banana plug wires.     
  
Theory:   
  
When two or more resistances are connected in series the equivalent resistance, RS is given by;

When two or more resistances are connected in parallel the equivalent resistance, RP is given   
by:





Procedure:  
  
1. Determine the values of the two resistors using [the resistor color code.](http://nearbus.net/wiki/index.php?title=File:Resistor_color_codes.jpg)       
  
2. Measure the values of the two resistors using the [digital multimeter](http://www.youtube.com/watch?v=bF3OyQ3HwfU) (DMM).  
  
3. Observe the tolerance values and record them in the data table.

4. Connect the three resistors in various combinations and obtain various values of resistances. Measure the equivalent resistances. Also calculate the equivalent resistances using the measured values for R1, R2, and R3. Identify the lowest and highest resistance values in the table.

|  |  |  |  |
| --- | --- | --- | --- |
| Resistor or combination diagram | Resistance Values | | Tolerance |
| Measured | Color-Code or Calculated |
| R1 |  |  |  |
| R2 |  |  |  |
| R1 andR2 in series |  |  | XXXXXXXXX  XXXXXXXXX  XXXXXXXXX  XXXXXXXXX  XXXXXXXXX |
| R1 andR2 in parallel |  |  | XXXXXXXXX  XXXXXXXXX  XXXXXXXXX  XXXXXXXXX  XXXXXXXXX |